Test object number          :2
Name of the channel         :Head impactor center / Y
Laboratory channel code     :D0HEAD0000PCDSYV
Customer channel code       :D0HEAD0000PCDSYV
Channel code                :D0HEAD0000PCDSYV
Location                    :NOVALUE
Direction                   :NOVALUE
Dimension                   :NOVALUE
Channel frequency class     :NOVALUE
Unit                        :mm
Reference system            :PC@T0
Transducer type             :NOVALUE
Transducer id               :NOVALUE
Transducer natural frequency:NOVALUE
Transducer damping ratio    :NOVALUE
Offset post test            :NOVALUE
Pre-filter type             :NOVALUE
Cut off frequency           :NOVALUE
Channel amplitude class     :NOVALUE
Reference channel           :implicit
Reference channel name      :NOVALUE
Data source                 :calculation
Data status                 :ok
Sampling interval           :0.001
Bit resolution              :NOVALUE
Time of first sample        :-0.028
Number of samples           :60
-14.3
-14.5
-13.1
-13.5
-12.9
-13.0
-12.7
-11.9
-11.3
-10.7
-10.2
 -9.2
 -8.8
 -8.2
 -7.6
 -6.3
 -6.0
 -4.5
 -4.5
 -3.8
 -3.3
 -2.1
 -1.9
 -1.2
 -0.7
 -0.1
 -0.2
  0.1
  0.0
  0.1
  0.9
  0.8
  1.6
  1.6
  1.9
  2.3
  3.1
  3.7
  4.0
  2.8
  3.6
  3.4
  4.7
  5.1
  5.7
  5.5
  5.3
  6.3
  5.9
  6.9
  7.1
  6.6
  7.3
  7.8
  8.8
  9.6
  9.0
  8.8
  9.2
  9.9
