Instrumentation standard    :ISO 6487 (1987) / SAE J211 (MAR95)
Comments                    :Channels 4-10 have another reference system
Number of channels          :10
Name of channel 001         :D0HEAD0000PCACXA / Kopf SP1 / X
Name of channel 002         :D0HEAD0000PCACYA / Kopf SP1 / Y
Name of channel 003         :D0HEAD0000PCACZA / Kopf SP1 / Z
Name of channel 004         :D0HEAD0000PCACRA / Kopf SP1 Res(X;Y;Z)
Name of channel 005         :D0HEAD0000PCDSXV / Head impactor center / X
Name of channel 006         :D0HEAD0000PCDSYV / Head impactor center / Y
Name of channel 007         :D0HEAD0000PCDSZV / Head impactor center / Z
Name of channel 008         :D0HEAD0000PCANXV / Head impactor center / Angle X
Name of channel 009         :D0HEAD0000PCANYV / Head impactor center / Angle Y
Name of channel 010         :D0HEAD0000PCANZV / Head impactor center / Angle Z
