Test object number          :2
Name of the channel         :Head impactor center / Angle Z
Laboratory channel code     :D0HEAD0000PCANZV
Customer channel code       :D0HEAD0000PCANZV
Channel code                :D0HEAD0000PCANZV
Location                    :NOVALUE
Direction                   :NOVALUE
Dimension                   :NOVALUE
Channel frequency class     :NOVALUE
Unit                        :degree
Reference system            :PC@T0
Transducer type             :NOVALUE
Transducer id               :NOVALUE
Transducer natural frequency:NOVALUE
Transducer damping ratio    :NOVALUE
Offset post test            :NOVALUE
Pre-filter type             :NOVALUE
Cut off frequency           :NOVALUE
Channel amplitude class     :NOVALUE
Reference channel           :implicit
Reference channel name      :NOVALUE
Data source                 :calculation
Data status                 :ok
Sampling interval           :0.001
Bit resolution              :NOVALUE
Time of first sample        :-0.028
Number of samples           :60
  1.9
  2.6
  0.9
  1.8
  1.8
  2.4
  3.4
  2.1
  2.5
  1.7
  3.7
  2.3
  4.5
  3.7
  4.6
  2.8
  3.9
  2.6
  3.1
  3.1
  2.7
  1.8
  0.5
  1.3
 -0.1
  0.0
  0.1
  0.4
 -0.1
 -0.4
 -0.2
 -1.5
 -2.6
 -1.6
 -1.6
 -2.7
 -3.4
 -2.8
 -3.1
 -1.1
 -3.0
 -1.6
 -3.6
 -4.8
 -5.7
 -4.9
 -6.0
 -7.0
 -6.8
 -6.7
 -8.0
 -6.9
 -6.7
 -9.0
-11.2
-11.7
 -7.6
 -8.6
-10.6
-11.8
