Test object number          :2
Name of the channel         :Head impactor center / Angle Y
Laboratory channel code     :D0HEAD0000PCANYV
Customer channel code       :D0HEAD0000PCANYV
Channel code                :D0HEAD0000PCANYV
Location                    :NOVALUE
Direction                   :NOVALUE
Dimension                   :NOVALUE
Channel frequency class     :NOVALUE
Unit                        :degree
Reference system            :PC@T0
Transducer type             :NOVALUE
Transducer id               :NOVALUE
Transducer natural frequency:NOVALUE
Transducer damping ratio    :NOVALUE
Offset post test            :NOVALUE
Pre-filter type             :NOVALUE
Cut off frequency           :NOVALUE
Channel amplitude class     :NOVALUE
Reference channel           :implicit
Reference channel name      :NOVALUE
Data source                 :calculation
Data status                 :ok
Sampling interval           :0.001
Bit resolution              :NOVALUE
Time of first sample        :-0.028
Number of samples           :60
  0.0
 -0.1
  0.1
 -0.1
  0.0
 -0.1
 -0.2
  0.0
 -0.1
  0.0
 -0.2
  0.0
 -0.3
 -0.1
 -0.2
  0.0
 -0.2
  0.0
 -0.1
  0.0
  0.0
  0.1
  0.2
  0.1
  0.4
  0.4
  0.3
  0.3
  0.0
 -1.1
 -3.2
 -5.4
 -7.8
-10.1
-12.1
-14.1
-15.9
-18.2
-20.5
-23.1
-25.4
-28.0
-30.2
-32.4
-34.6
-36.7
-38.5
-40.3
-42.0
-43.6
-45.0
-46.6
-48.0
-49.2
-50.2
-51.4
-53.1
-54.4
-55.6
-56.9
