Test object number          :2
Name of the channel         :Head impactor center / Z
Laboratory channel code     :D0HEAD0000PCDSZV
Customer channel code       :D0HEAD0000PCDSZV
Channel code                :D0HEAD0000PCDSZV
Location                    :NOVALUE
Direction                   :NOVALUE
Dimension                   :NOVALUE
Channel frequency class     :NOVALUE
Unit                        :mm
Reference system            :PC@T0
Transducer type             :NOVALUE
Transducer id               :NOVALUE
Transducer natural frequency:NOVALUE
Transducer damping ratio    :NOVALUE
Offset post test            :NOVALUE
Pre-filter type             :NOVALUE
Cut off frequency           :NOVALUE
Channel amplitude class     :NOVALUE
Reference channel           :implicit
Reference channel name      :NOVALUE
Data source                 :calculation
Data status                 :ok
Sampling interval           :0.001
Bit resolution              :NOVALUE
Time of first sample        :-0.028
Number of samples           :60
 -7.5
 -7.6
 -7.4
 -7.4
 -6.6
 -6.4
 -7.0
 -6.0
 -6.2
 -5.7
 -5.7
 -4.3
 -5.0
 -5.5
 -5.3
 -4.4
 -4.3
 -3.8
 -3.4
 -3.0
 -2.9
 -2.8
 -2.0
 -1.5
 -1.2
 -1.0
 -1.0
 -0.6
  0.0
  0.0
  0.9
  0.5
  1.5
 -1.0
 -1.2
 -0.3
 -2.6
 -2.6
 -4.7
 -6.4
 -8.2
 -9.6
-10.8
-12.1
-14.3
-18.0
-19.4
-22.3
-24.9
-28.2
-30.5
-33.6
-35.8
-37.7
-40.6
-43.1
-47.6
-50.6
-53.2
-55.3
