Test object number          :2
Name of the channel         :Head impactor center / X
Laboratory channel code     :D0HEAD0000PCDSXV
Customer channel code       :D0HEAD0000PCDSXV
Channel code                :D0HEAD0000PCDSXV
Location                    :NOVALUE
Direction                   :NOVALUE
Dimension                   :NOVALUE
Channel frequency class     :NOVALUE
Unit                        :mm
Reference system            :PC@T0
Transducer type             :NOVALUE
Transducer id               :NOVALUE
Transducer natural frequency:NOVALUE
Transducer damping ratio    :NOVALUE
Offset post test            :NOVALUE
Pre-filter type             :NOVALUE
Cut off frequency           :NOVALUE
Channel amplitude class     :NOVALUE
Reference channel           :implicit
Reference channel name      :NOVALUE
Data source                 :calculation
Data status                 :ok
Sampling interval           :0.001
Bit resolution              :NOVALUE
Time of first sample        :-0.028
Number of samples           :60
-304.4
-294.1
-282.0
-271.9
-261.1
-250.8
-240.9
-229.0
-218.6
-207.2
-198.1
-186.1
-177.2
-165.6
-155.5
-143.2
-133.3
-121.3
-110.8
 -99.9
 -88.8
 -77.1
 -65.0
 -54.8
 -42.7
 -31.8
 -21.0
 -10.5
   0.0
   9.1
  16.4
  23.7
  30.1
  34.5
  38.9
  43.4
  47.6
  49.3
  51.6
  51.0
  53.8
  53.0
  54.7
  55.3
  55.8
  55.5
  54.7
  55.0
  53.5
  52.9
  52.1
  49.7
  47.3
  46.4
  46.5
  44.5
  40.7
  39.4
  38.5
  36.2
