Test object number          :2
Name of the channel         :Head impactor center / Angle X
Laboratory channel code     :D0HEAD0000PCANXV
Customer channel code       :D0HEAD0000PCANXV
Channel code                :D0HEAD0000PCANXV
Location                    :NOVALUE
Direction                   :NOVALUE
Dimension                   :NOVALUE
Channel frequency class     :NOVALUE
Unit                        :degree
Reference system            :PC@T0
Transducer type             :NOVALUE
Transducer id               :NOVALUE
Transducer natural frequency:NOVALUE
Transducer damping ratio    :NOVALUE
Offset post test            :NOVALUE
Pre-filter type             :NOVALUE
Cut off frequency           :NOVALUE
Channel amplitude class     :NOVALUE
Reference channel           :implicit
Reference channel name      :NOVALUE
Data source                 :calculation
Data status                 :ok
Sampling interval           :0.001
Bit resolution              :NOVALUE
Time of first sample        :-0.028
Number of samples           :60
 -0.9
 -1.3
 -1.3
 -1.5
 -0.8
 -0.8
 -1.7
 -0.8
 -1.2
 -0.9
 -1.2
  0.2
 -0.8
 -1.7
 -1.7
 -1.1
 -1.1
 -1.0
 -0.8
 -0.6
 -0.8
 -1.1
 -0.6
 -0.2
 -0.3
 -0.4
 -0.7
 -0.4
  0.0
  0.1
  0.8
  0.2
  1.4
 -1.0
 -0.5
  1.7
  0.2
  1.9
  1.1
  1.0
  0.7
  1.3
  2.1
  3.1
  3.1
  1.3
  3.0
  2.4
  2.7
  1.7
  2.7
  2.5
  3.8
  5.7
  5.8
  6.6
  4.2
  4.4
  5.2
  7.0
