* Auto-generated testbench for inrush analysis: U6 (LDO)
* Output: 5.0V, 120.0µF total capacitance
* Soft-start: 0.5ms ramp

* Voltage source with linear ramp (soft-start) — 10us delay before ramp
Vreg ramp 0 PWL(0 0 10u 0 510u 5.0)
* Regulator output impedance
Rout ramp out 100m

* Output capacitors
C7 out 0 10u
C3 out 0 100u
C8 out 0 10u

.control
tran 1u 1.5m
let i_out = abs(i(Rout))
let i_peak = vecmax(i_out)
let t_peak = i_out[vecmin(abs(i_out - i_peak))]
meas tran v_settled find v(out) at=1.35m
echo "i_peak=$&i_peak t_peak=$&t_peak v_settled=$&v_settled v_target=5.0 r_out=0.1" > analysis/spice_runs/inrush_idx0.out
quit
.endc

.end
