=== stdout ===

Note: No compatibility mode selected!


Circuit: * auto-generated testbench for inrush analysis: u6 (ldo)

Doing analysis at TEMP = 27.000000 and TNOM = 27.000000

Using SPARSE 1.3 as Direct Linear Solver

Initial Transient Solution
--------------------------

Node                                   Voltage
----                                   -------
ramp                                         0
out                                          0
vreg#branch                                  0


No. of Data Rows : 1517
v_settled           =  5.00000e+00
ngspice-46 done

=== stderr ===

Error: no such function as i,
    or i(rout) is not available.
Error: RHS "abs(i(rout))" invalid
Warning from checkvalid: vector i_out is not available or has zero length.
Error: RHS "vecmax(i_out)" invalid
Warning from checkvalid: vector i_out is not available or has zero length.
Error: RHS "i_out[vecmin(abs(i_out - i_peak))]" invalid
Error: &i_peak: no such variable.
Error: &t_peak: no such variable.

