(footprint "MountingHole_2.7mm_M2.5_DIN965" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (descr "Mounting Hole 2.7mm, no annular, M2.5, DIN965")
  (tags "mounting hole 2.7mm no annular m2.5 din965")
  (attr exclude_from_pos_files exclude_from_bom)
  (fp_text reference "REF**" (at 0 -3.35) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp b8c057d5-dc17-453d-912f-05b30d7e612e)
  )
  (fp_text value "MountingHole_2.7mm_M2.5_DIN965" (at 0 3.35) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 1a1b385a-cb8d-4557-99fd-e5782d36c05f)
  )
  (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp e08aae11-f655-4941-b438-d9802e1d4b1f)
  )
  (fp_circle (center 0 0) (end 2.35 0)
    (stroke (width 0.15) (type solid)) (fill none) (layer "Cmts.User") (tstamp 66aea7f3-1bbe-4964-a920-8bc4d04f21ec))
  (fp_circle (center 0 0) (end 2.6 0)
    (stroke (width 0.05) (type solid)) (fill none) (layer "F.CrtYd") (tstamp 88f42438-87c5-4c9d-966a-6d3ad861acc9))
  (pad "" np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers "F&B.Cu" "*.Mask")
    (solder_mask_margin 1.3) (clearance 1.3) (tstamp 7388b760-277c-4b82-bf7a-9ed81224c843))
)
