(footprint "MTCONN_UBAF30-D2011"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "USB3 Stacked type A socket")
	(tags "USB3 TypeA")
	(property "Reference" "REF**"
		(at 0 -0.5 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "159e0420-4325-4168-86b6-a228ae385b74")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "MTCONN_UBAF30-D2011"
		(at 0 1 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "030d9eed-d060-4fb7-a3e5-dd631c9878c2")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" "MTCONN_UBAF30-D2011"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "ef8a18e9-0883-48e2-8681-d9035c0f4a3e")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "ef5e3cea-3b46-42f1-a71e-6619c5c184ad")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "64766762-f58d-495a-8fe2-957f1bc32c95")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(attr through_hole)
	(fp_line
		(start -6.89 -7.86)
		(end 6.89 -7.86)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "1aaca878-b95d-40c0-a6e7-e51d7ea87a6c")
	)
	(fp_line
		(start -6.89 9.64)
		(end -6.89 2)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "2e8f5299-7f88-46a5-a8cb-1a0fed2366f9")
	)
	(fp_line
		(start -6.89 9.64)
		(end 6.89 9.64)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "57e0bd81-dcb8-4586-9f3d-f7fad7eb46f9")
	)
	(fp_line
		(start 6.89 2)
		(end 6.89 9.64)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "be9518e5-64b7-488c-b8e0-57dbc0b31ecf")
	)
	(fp_line
		(start -6.89 -7.86)
		(end -6.89 9.64)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "ed80fa79-747c-43b5-9b38-fb5bd42e26f7")
	)
	(fp_line
		(start -6.89 9.64)
		(end 6.89 9.64)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "c0dacdc1-bf02-49df-9de9-fb872c40583a")
	)
	(fp_line
		(start 6.89 -7.86)
		(end -6.89 -7.86)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "8cd79c52-f48b-4e66-a52b-72a42cc9b835")
	)
	(fp_line
		(start 6.89 9.64)
		(end 6.89 -7.86)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "7e13241e-25aa-48d7-8150-c41ff27ccc60")
	)
	(fp_text user "${REFERENCE}"
		(at 0 2.5 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "fb08ffad-6464-4b99-bca1-78f476d9fe28")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "10" thru_hole circle
		(at -6.57 -5.68)
		(size 3.1 3.1)
		(drill 2.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "bb9918bd-f910-4902-ae20-97a3e82279c6")
	)
	(pad "10" thru_hole circle
		(at -6.57 0)
		(size 3.1 3.1)
		(drill 2.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "123c45e8-8d30-431c-9aba-0a7ac963657a")
	)
	(pad "10" thru_hole circle
		(at 6.57 -5.68)
		(size 3.1 3.1)
		(drill 2.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "198bdd97-4623-4da9-8a84-0734fe1062a4")
	)
	(pad "10" thru_hole circle
		(at 6.57 0)
		(size 3.1 3.1)
		(drill 2.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "ca8e5715-c125-44c3-9def-e42736e52986")
	)
	(pad "A1" thru_hole circle
		(at -3.5 -2)
		(size 1.1 1.1)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "d24ba20f-b5c5-46a6-acbe-e1d66cd453f3")
	)
	(pad "A2" thru_hole circle
		(at -1 -2)
		(size 1.1 1.1)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "318fee4e-d435-4430-a906-50f9661f31e4")
	)
	(pad "A3" thru_hole circle
		(at 1 -2)
		(size 1.1 1.1)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "def50e31-8215-4c92-94e7-1aa356c381da")
	)
	(pad "A4" thru_hole circle
		(at 3.5 -2)
		(size 1.1 1.1)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "93613739-6dd7-41f2-93cc-ca47ef8f1524")
	)
	(pad "A5" thru_hole circle
		(at 4 -3.5)
		(size 1.1 1.1)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "baceeda7-bade-4256-8bbb-c28f24f4ed4f")
	)
	(pad "A6" thru_hole circle
		(at 2 -3.5)
		(size 1.1 1.1)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "a5103b18-1ab3-4c42-a2a8-a012dcc97ba9")
	)
	(pad "A7" thru_hole circle
		(at 0 -3.5)
		(size 1.1 1.1)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "a4630606-90f5-48f4-b947-2b116f3c305c")
	)
	(pad "A8" thru_hole circle
		(at -2 -3.55)
		(size 1.1 1.1)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "b95e4631-c4e4-4f3f-bb43-563701a5cf2c")
	)
	(pad "A9" thru_hole circle
		(at -4 -3.5)
		(size 1.1 1.1)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "a0d2d040-4f0a-4784-b768-cf0168224cc0")
	)
	(pad "B1" thru_hole circle
		(at -3.5 -5.2)
		(size 1.1 1.1)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "9b5ced6a-fbec-4cd9-a3eb-b178c0b3e470")
	)
	(pad "B2" thru_hole circle
		(at -1 -5.2)
		(size 1.1 1.1)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "32f8e1ec-e58b-4513-8a59-443ac2bcbedd")
	)
	(pad "B3" thru_hole circle
		(at 1 -5.2)
		(size 1.1 1.1)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "f50ee2b6-ebf4-4e4e-be8d-4d16045d962d")
	)
	(pad "B4" thru_hole circle
		(at 3.5 -5.2)
		(size 1.1 1.1)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "c097ec24-fe9e-4d95-aa42-d6a7782bcaf1")
	)
	(pad "B5" thru_hole circle
		(at 4 -6.7)
		(size 1.1 1.1)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "9f4d9b10-b0ee-43e0-98b1-7b6189db7ee7")
	)
	(pad "B6" thru_hole circle
		(at 2 -6.7)
		(size 1.1 1.1)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "5a22bd4a-ac05-446f-87ba-ac485a78e924")
	)
	(pad "B7" thru_hole circle
		(at 0 -6.7)
		(size 1.1 1.1)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "e20a5ea4-e4eb-49a0-a32f-03c3d6b4ce25")
	)
	(pad "B8" thru_hole circle
		(at -2 -6.75)
		(size 1.1 1.1)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "2b9dcb68-55a6-4469-99c6-e7842323b544")
	)
	(pad "B9" thru_hole circle
		(at -4 -6.7)
		(size 1.1 1.1)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "c023e606-9337-46f2-b835-98b4401d6a0a")
	)
	(model "${KIPRJMOD}/CM5IO.3dshapes/USB3stacked.STEP"
		(offset
			(xyz 0 -0.6 8.5)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -90 0 0)
		)
	)
)
